**Draper Adds IP Option for Screens and Lifts**

**(Spiceland, Ind.) –** Draper is making it easier than ever to add projection screens and projector lifts to AV Over IP.

The new LVC-IP Bridge converts command strings sent over IP to serial strings, making it possible to be connected to an IP network. Configuration is done using the built-in buttons and display.

“This a great wat to get Draper electric screens and lifts onto your network because it simplifies the process,” said Jim Hoodlebrink, AV Consultant Relations and Pro AV Products for Draper. “We wanted to make it as easy as possible, and since all programming is done on the device, you don’t have to hook up a laptop to do it.”

Mounting hardware for the 4-7/8” x 3” x 1” device is included. A Draper LVC low voltage module is also required, and sold separately.

For more information visit booth W1001 at InfoComm 2024, or go to **draperinc.com/projectionscreens/productdetailaccessories/1137**.

**About Draper**Draper, Inc. creates core, advanced, and tailored solutions for the professional audiovisual marketplace, including projection screens, custom AV mounts, structures, enclosures and lifts, as well as window shades and video conferencing solutions. The family-owned and operated business was established in 1902, and markets through a network of dealers and distributors to the commercial, architectural, education, and residential markets. To learn more, visit [www.draperinc.com](http://www.draperinc.com).

**Media Contact**Terry Coffey  
Phone: 765-856-1230  
E-mail: [**tcoffey@draperinc.com**](mailto:tcoffey@draperinc.com)Website: [**www.draperinc.com**](http://www.draperinc.com)